ACOUSTIC PRODUCTS

LINEA SLATTED ACOUSTIC PANELS
K13/170 NBS TECHNICAL SPECIFICATION

ACOUSTIC PANELS TO: _________________________________________

Refer to drawings: ________________________________________________________________

Manufacturer and reference: LINEA timber slatted acoustic wall/ceiling panels, design reference ………………… by 

Acoustic Products Ltd

70C High Street
Whitstable
Kent
CT5 1BB
Tel
01227 281140

Fax
01227 281141

Email
enquiries@acoustic-products.co.uk
Slat Size/Spacing:      Slats …… mm wide x …….mm high spaced at …. mm centres

Panel Substrate: 
Solid wood in …………. Impregnated to give a EN B-s2,d0 fire rating with “natural” finish
Additional Surface Finish:  None/Colour waxed to imitate ……… hardwood appearance
Panel sizes & quantities – Pre fabricated units in standard sizes of 1880mm x 600mm and/or 1265mm x 600mm
Installation:               In accordance with the manufacturer’s recommendations all as detailed in the LINEA Installation Manual available to download at: www.acoustic-products.co.uk/movable-wall-technical-downloads
