ACOUSTIC PRODUCTS LTD

SERIES GS 100 DOUBLE GLAZED MOVING WALL

L20/540 NBS TECHNICAL SPECIFICATION
SLIDING FOLDING PARTITIONS TO:________________________
Refer to drawing no(s): ___________________________________________________________

Manufacturer and reference:  Series GS 100 Double Glazed Moving Wall by 


Acoustic Products Ltd

70C High Street

Whitstable

Kent

CT5 1BB
Tel
01227 281140

Fax
01227 281141

Email: enquiries@acoustic-products.co.uk
Characteristics:  
Manually operated modular aluminium framed panel system with easy operation internal locking mechanism.  Top and bottom retractable seals.

Passdoors:  
Single full height door hinged to a wall jamb.

Finishes:  
100 mm overall thickness panel with internal aluminium frame, 6 mm thick toughened glass both sides, painted frit border

Panel Edge Trims: 

Concealed satin anodised aluminium 

Furniture:  


Removable winding handle

Track and Roller System:
Two point suspension for offset stacking, heavy duty extruded aluminium top track with integral ceiling trim, powder coat finish white.  No floor track.

Acoustic Rating:  

Rw 41 dB

