ACOUSTIC PRODUCTS

TOPAKUSTIK ACOUSTIC PLANKS

K13/170 NBS TECHNICAL SPECIFICATION

ACOUSTIC PLANKS TO: _________________________________________

Refer to drawings: ________________________________________________________________

Manufacturer and reference: Topakustik acoustic planks, design reference ………………… by 

Acoustic Products Ltd

70C High Street

Whitstable

Kent

CT5 1BB
Tel
01227 281140

Fax
01227 281141

Email
enquiries@acoustic-products.co.uk

Panel Substrate: 
16 mm thick DIN B2 non fire rated MDF/16 mm thick EN B s1 d0 fire rated 

MDF (European equivalent to BS Class O) MDF/DIN A1 “RESAP” gypsum/ chipboard non combustible composite

Front Surface Finish:   ……………………………veneer with DIN B2 non fire rated factory

 applied lacquer finish/DIN B1 fire retardant factory applied 

 lacquer finish




 Factory spray painted to RAL/NCS colour reference ……………………………..




 Melamine colour/design reference …………………………..




 Laminate colour/design reference ……………………………

Edges: 

 Long edges tongued and grooved, ends square cut in raw 

 MDF

Rear:


 Black acoustic fleece on rear surface covering rear perforations

Plank sizes: 

3640mm or 4080m standard lengths + or -3 mm x 128 mm cover width

Rear:


 Black acoustic fleece on rear surface covering rear perforations

Acoustic Insulation:
30 mm thick mineral wool (40-60 kgs/cu M, 2.5-3.75 pcf) behind panels

Installation:            The planks to be suspended using any proprietary MF style suspension system 

        finishing at a 24-26 mm T-bar profile spaced at 600 mm centres. The 

        Topakustik planks to be fixed to these T-bars using n’H Akustik “Turning Clips” 

        which twist on to the T-bars and have a lower projection which locates into a 

        special additional groove in the edge of the Topakustik planks.

