ACOUSTIC PRODUCTS

TOPAKUSTIK CABINET DOORS
K13/170 NBS STYLE TECHNICAL SPECIFICATION

ACOUSTIC CABINET DOORS TO: ________________________________

Refer to drawings: ________________________________________________________________

Manufacturer and reference: Topakustik cabinet doors, face design reference ………………… by 

Acoustic Products Ltd

70C High Street

Whitstable

Kent

CT5 1BB
Tel
01227 281140

Fax
01227 281141

Email
enquiries@acoustic-products.co.uk

Door Construction: 
 TYPE RK/SW/DUPLEX
Front Surface Finish:   ……………………………veneer with DIN B2 non fire rated factory

 applied lacquer finish/DIN B1 fire retardant factory applied 

 lacquer finish




 Factory spray painted to RAL/NCS colour reference ……………………………..




 Melamine colour/design reference …………………………..




 Laminate colour/design reference ……………………………

Edges: 

 Square cut raw MDF/Veneered to match/Factory

 spray painted to match/Melamine to match/Laminate to match.

Panel sizes & quantities: ………………………………………… 

Installation:               Method of fixing cabinet doors: in accordance with manufacturer’s 
                                recommendations

