ACOUSTIC PRODUCTS

TOPPERFO ACOUSTIC PANELS

K13/170 NBS TECHNICAL SPECIFICATION

ACOUSTIC PANELS TO: _________________________________________

Refer to drawings: ________________________________________________________________

Manufacturer and reference: Topperfo acoustic panels, design reference ………………… by 

Acoustic Products Ltd

70C High Street

Whitstable

Kent

CT5 1BB
Tel
01227 281140

Fax
01227 281141

Email
enquiries@acoustic-products.co.uk

Panel Substrate: 
 16 mm thick DIN B2 non fire rated MDF/16 mm thick DIN B1 fire retardant 

 MDF/DIN A1 “RESAP” gypsum chipboard non combustible composite

Front Surface Finish:   ……………………………veneer with DIN B2 non fire rated factory

 applied lacquer finish/DIN B1 fire retardant factory applied 

 lacquer finish




 Factory spray painted to RAL/NCS colour reference ……………………………..




 Melamine colour/design reference …………………………..




 Laminate colour/design reference ……………………………

Edges: 

 Square cut raw MDF/Square cut ”RESAP”/Veneered to match/Factory

 spray painted to match/Melamine to match/Laminate to match.

Rear:


 Black acoustic fleece on rear surface covering rear perforations

Panel sizes & quantities: ………………………………………… (DIN B2 & B1 MDF max. panel size 3640mm x 1216 mm/DIN A1 “RESAP” max. panel size 2976 mm x 992 mm”, cut to specific sizes in the factory subject to waste surcharge; max. panel widths If G or Z suspension systems required:  500 mm wide if G-suspension or 640 mm wide if Z-suspension)
Acoustic Insulation:
30 mm thick mineral wool (40-60 kgs/cu M, 2.5-3.75 pcf) behind panels

Installation:                The long panel edges to be profiled to suit either “Type G” suspension 

                                 (where every panel is removable – max. 500 mm panel width) 

or “Type Z” suspension (where every other panel is removable – max panel  width 640 mm). Main U-Channel support profiles (available in  

            3750 mm lengths) to be installed at 1200 mm centres, “Type G” or “Type

            Z” profiles (available in 5000 mm lengths) to be clamped at right angles to

            the main U-Channel support profiles (at centres to match the panel width).

